MODEL 1 – Ducato Goods Transport – OVERVIEW - TEXTS

1. SECTION TITLE

RANGE AND LOAD CAPACITY

*A huge variety of combinations, for endless transport solutions*

2. BLOCK 2

(ONLY TEXT)

**FLEXIBILITY**

*Custom-made solutions by authorised outfitters*

**A fully-equipped mobile workshop in your van**

For on-site technical and mechanical assistance, fitted with an aluminium loading platform and internal shelving.

**Refrigeration/Isothermal outfit**

For carrying food and medicine, in compliance with the applicable standards in force, insulated with or without refrigerator.

3. BLOCK 3

(FULL TEXT LEFT)

**ACCESSIBILITY**

You can make the most of every last centimetre of space when loading your goods

The **sliding side doors** are available in **2 widths**, **1075** and **1250** mm, and **2 heights**, **1485** and **1755** mm.

4 BLOCK 4

(ONLY TEXT)

And not only that:

* theupper **slide rail** is designed to facilitate opening and closing
* the **suitcase-style *handles***are easy to grip.

A **second sliding side door** - on the right hand side - is available on request.

The **load compartment** is **extremely easy to access** via the rear door:

* the door is **over 1.5 m high on the low roof version**, almost **1.8 m on the high roof version**, and over **2 m on the super high roof**, truly a **record height** - meaning you have no need to tilt your goods to load them;

two opening options **180°** and **270°**, for easier movement around the vehicle in confined spaces.

5. BLOCK 5

(ONLY TEXT)

**Self-levelling suspension**

To keep you **level at all times**, irrespective of load weight and arrangement, thus increasing safety and **driving comfort.**

Allows you **to raise or lower the load platform** when the vehicle is parkedin order to:

* make the handling of your goods easier

improve the ramp angle or pass over an obstacle beneath the vehicle

6. BLOCK 6

(FULL RIGHT TEXT)

**VAN**

***Generous in volume, generous in capacity***

* **3 wheelbases**, **4** lengths, **3** heights.
* **8 volume options**, from **8** to **17** m3.
* **Sliding side door** and **rear door both available in 3 different size options**.
* GVW : 2600 to 4250 kg
* **payload** from **1000 to 2200 kg**.
* **Maximum permitted** axle loads **up to 2100 kg** on the front and **up to 2500 kg** on the rear.

**2** different **mechanical structures**, **the Ducato** and **the Ducato Maxi with reinforced suspension and 16”** wheels.

7. BLOCK 7

(ONLY TEXT)

**LOAD COMPARTMENT**

The load compartment is square and even, and every last bit of space can be used:

* it **is** between **267** and **407 cm long**
* and **up** to **166** to **217 cm high**
* the **width between the wheel arches** is **142 cm,** meaning120 cm Euro pallets can be loaded quicklyand **easily**
* the flatbed can be protected by a highly resistant plywood cover
* the interior walls can be covered in thermoformed plastic panels
* to fix and retain the load in place, **4 securing hooks** are available at the sides of the load compartment, as well as several anchoring points on the flatbed
* a bright interior is guaranteed by the 15 W ceiling lights - **an additional 12 V power point inside the load compartment is also available on request, as well as a removable rechargeable ceiling light.**

**The partition** between the load compartment and the passenger compartment may be panelled or glazed with sliding glass.

**Panel/glazed/semi-glazed Van**

**GVW**: 2600 to 3500 kg

**Capacity:** 830 to 1655 Kg

**Volume**: 8 to 15 m³

**Wheelbase:** 3000, 3450, 4035 mm

**External dimensions**:

- Length: 4963 to 5998 mm

- Height: 2254 to 2764 mm

- Width: 2050 mm

**Load compartment dimensions:**

- Height: 1.662 m to 2.172 m

- Width: 1.870 m

- Width between wheel arches: 1.422 m

- Length: 2.670 m to 3.705 m

**No. of seats in cab:** 2/3

**Panel/glazed/semi-glazed Maxi Van**

**GVW**: 3500 to 4200 kg

**Capacity:** 1330 to 2110 Kg

**Volume**: 10 to 17 m³

**Wheelbase:** 3450, 4035 mm

**External dimensions**:

- Length: 5413 to 6363 mm

- Height: 2539 to 2779 mm

- Width: 2050 mm

**Load compartment dimensions:**

- Height: 1.932 m to 2.172 m

- Width: 1.870 m

- Width between wheel arches: 1.422 m

- Length: 3.120 m to 4.070 m

**No. of seats in cab:** 2/3

8. BLOCK 8

(FULL RIGHT TEXT)

**CREW CAB VAN**

***Designed to carry your crew***

* **3 lengths**, 2 heights
* double row of seats to seat **up to 7 people**
* **GVW options** from **3300** to **3500 kg**
* **payload** from 1480 to 2880 kg
* **volumes of 3.6 - 8.3**
* designed to **make room for your crew**

**pipe storage compartment of 1.1** m under the rear seats

9. BLOCK 9

(ONLY TEXT)

**Crew Cab Van**

**GVW**: 3300 to 3500 kg

**Payload**:  1194 to 1489 kg

**Volume**: from 3.6 to 8.3 m3

**Wheelbase**: 3000, 4035 mm

**External** **dimensions**:

- Length: 4963 to 6363 mm

- Height: 2254 to 2539 mm

- Width: 2050 mm

**Load** **compartment** **dimensions**:

- Height: 1.662 m to 1.932 m

- Width: 1.87 m

- Width **between** wheel arches: 1.42 m

- Length: 1.48 m to 2.88 m

**No. of seats in cab**: 6/7

10. BLOCK 10

(FULL RIGHT TEXT)

**TRUCK**

***Functionality, capacity, practicality and comfort***

* **4 wheelbases, 5 lengths.**
* **2 types of cab, single and double.**
* **GVW from 3000 to 4250 kg.**
* **maximum permitted load of 2100 kg on the front axle and up to 2500 kg on the rear axle**
* **8 body dimensions with surface areas from 4.9 to 8.5 m2.**

**2 different mechanical structures, the Ducato and the Ducato Maxi with reinforced suspension and 16” wheels.**

11. BLOCK 11

(ONLY TEXT)

**LOAD COMPARTMENT**

The sturdy and reliable original flatbeds are produced using **state of the art materials and technologies**:

* **the load platform, 2 m** wide and **2.8** to **4.2 m** long, is crafted from Scandinavian timber and treated with phenol resins to ensure an anti-slip surface which is highly resistant to abrasion
* **the side boards are made of aluminium profiles**, making them undeformable and light for optimised payload, **40 cm high** and fitted with an access step.

The **load surface** ranges from **4.9** to **8.5** m2.

**Trucks**

**GVW**: 3000 to 3500 kg

**Capacity:** 1110 to 1625 Kg

**Load area**: 5.7 to 8.5 m²

**Wheelbase:** 3000, 3450, 4035 and 4035 XL mm

**External dimensions**:

- Length: 5293 to 6693 mm

- Height: 2424 mm

- Width: 2100 mm

**Flatbed interior dimensions:**

- Width 2.034 m

- Length: 2.798 m to 4.198 m

- Side height: from 0.4 m

**No. of seats in cab:** 2/3

**Maxi Truck**

**GVW**: 3000 to 42.250 kg

**Capacity:** 1110 to 2120 Kg

**Load area**: 6.6 to 8.5 m²

**Wheelbase:** 3450, 3800, 4035 and 4035 XL mm

**External dimensions**:

- Length: 5743 to 6693 mm

- Height: 2424 mm

- Width: 2100 mm

**Flatbed interior dimensions:**

- Width 2.034 m

- Length: 3.428 m to 4.198 m

- Side height: from 0.4 m

**No. of seats in cab:** 2/3

**Crew Cab Truck**

**GVW**: 3300 to 3500 kg

**Capacity:** 1225 to 1535 Kg

**Load area**: 4.9 to 5.9 m²

**Wheelbase:** 3450, 4035 mm

**External dimensions**:

- Length: 5738 to 6228 mm

- Height: 2424 mm

- Width: 2100 mm

**Flatbed interior dimensions:**

- Width: 2 m

- Length: 2.398 m to 2.888 m

- Side height: from 0.4 m

**No. of seats in cab:** 6/7

12. BLOCK 12

(FULL RIGHT TEXT)

**TRUCK WITH FLAT-BED TIPPER**

***Designed, built and guaranteed directly by Fiat Professional***

12. BLOCK 12

(ONLY TEXT)

* **2 wheelbases**
* **GVW options** from **3300** to 3500 kg
* **payload** from 927 to 1162 kg
* flat-bed tipper with a surface area of between 5.1 and 6.8 m2

**solid steel structure** to withstand the toughest working conditions.

**LOAD COMPARTMENT**

The sturdy and reliable original flatbeds were designed to simplify work in the toughest conditions:

* **the load bed**, which is **2 m** wide and between **2.5** and **3.3 m** long, is made of sturdy steel
* **the sturdy aluminium side boards** are **39 cm high** and fitted with a practical access step.

The **load surface** ranges from **5.1** to **6.8** m2.

**Truck with flat-bed tipper**

**GVW**: 3300 to 3500 kg

**Payload**: 927 to 1162 kg

**Load area**: from 5.1 to 6.8 m2

**Wheelbase**: 3000, 4035 mm

**External dimensions**:

- Length: 5028 to 6123 mm

- Width: 2100 mm

**Load compartment dimensions**:

- Side height: 0.39 m

- Width: 2.040 m

- Length: 2.525 m to 3.325 m

**No. of seats in cab**: 2/3

**Tipper**

**GVW**: 3300 to 3500 kg

**Payload**: 772 to 972 kg

**Load area**: 5.6 m2

**Wheelbase**: 4035 mm

**External dimensions**:

- Length: from 6123 mm

- Width: 2100 mm

**Load compartment dimensions**:

- Side height: 0.320 m

- Width: 2.040 m

- Length: 2.750 m

**No. of seats in cab**: 6/7